|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Service  UUID | NAME | PROPERTIES | UUID | LENGTH | DESCRIPTION |
| 1803 | Link Loss | READ, WRITE | 2A06 | 1 | Alert Level |
| 1802 | Immediate Alert | WRITE  NO RESPONSE | 2A06 | 1 | Alert Level |
| 1804 | TX Power | READ | 2A07 | 1 | TX Power Level（0x00） |
| 2800 | Battery Service | READ, NOTIFY | 2A19 | 1 | Battery Level（0-100） |
| Device Information | READ | 2A29 | 18(MAX) | Manufacturer Name String |
| READ | 2A24 | 18(MAX) | Model Number String |
| READ | 2A26 | 18(MAX) | Firmware Revision String |
| READ | 2A28 | 18(MAX) | Software Revision String |
| READ | 2A23 | 8(MAX) | System ID |
| READ | 2A50 | 7(MAX) | PnP ID |
| FEF5 |  |  |  |  |  |

///Alert Level Values

enum

{

PROXR\_ALERT\_NONE,

PROXR\_ALERT\_MILD,

PROXR\_ALERT\_HIGH,

};